Head for High Temperature Applications

|  |  |
| --- | --- |
| 17260-35 | 11 - 35**°**C |