Fully-lugged Gear Operated Butterfly Valve PN16 WRAS Approved

|  |  |
| --- | --- |
| HV-BF-FLG-06 | 2" |
| HV-BF-FLG-07 | 2½" |
| HV-BF-FLG-08 | 3" |
| HV-BF-FLG-09 | 4" |
| HV-BF-FLG-10 | 5" |
| HV-BF-FLG-11 | 6" |
| HV-BF-FLG-12 | 8" |
| HV-BF-FLG-13 | 10" |
| HV-BF-FLG-14 | 12" |